Asteroids Signatures, ROM all -02 only.


Good RAM, ROM, and board will stay in self test assumed.


Board A034986 (gap in middle)





DIP switches don't matter


Watchdog - not disabelled


Dag ON


Self Test ON


Should hear a "Beep"





Start (+) A10 -1


Stop (-) A10-1


Clock (-) Phase 2 test point





Signatures


Vcc - 3H16


Gnd - 0000





IC-F7 74LS273 Vector Generator Memory DATA Latches


1-3H16	20-3H16


2-A82A	19-0000


3-78F2	18-H6P1


4-453U	17-A8UF


5-0000	16-0000


6-6U88	15-6P3H


7-1394	14-649P


8-4H1H	13-0028


9-01C2	12-F610


10-GND	11-3UF8





IC-H7 LS273 Vector Generator Memory DATA Latches


1-1P8C	20-VCC


2-5415	19-5415


3-78F2	18-H6P1


4-453U	17-A8UF


5-5416	16-5415


6-5415	15-5415


7-1394	14-649P


8-4H1H	13-0028


9-00H9	12-5415


10-0000	11-3F79





IC-J7 LS273 Vector Generator Memory DATA Latches


IC-K7 LS273 Vector Generator Memory DATA Latches


.....





IC-F6 LS157 Vector Timer


1-3H16	16-VCC


2-3H16	15-0000


3-6U88	14-0000


4-6U88	13-6P3H


5-0000	12-6P3H


6-01C2	11-0000


7-01C2	10-F610


8-GND	9-F610





IC-M7 LS175


1-3H16	16-VCC


2-0000	15-0000


3-3H16	14--3H16


4-66U5	13-66U5


5-0000	12-66U5


6-3H16	11-3H16


7-0000	10-0000


8-GND	9-U40A





IC-E7 LS42 


1-F7A2	16-VCC


2-3H16	15-6P3H


3-3H16	14-6U88


4-3H16	13-F610


5-3H16	12-01C2


6-3H16	11-953F


7-3H16	10-3H16


8-GND	9-UC06





IC-D7 LS161`


7-3991


15-P327





IC-C7 LS161


15-3HU5





IC-B7 LS161 Vector Timer


15-0000





IC-D4 LS74 Vector Generator Program Counter	


2-AFH8


6-532C





IC-K6 LS08


8-3H14


9-3H16


10-3H14





IC-K6 LS191


5-6P3H


3,2 - UNSTABLE





IC-F5 LS193


1-6P3H	16-VCC


2-P3AC	15-693H


3-P371	14-0000


4-3H16	13-3H16


5-7F23	12-3H16


6-FP5A	11-AFH8


7-0000	10-6P3H


8-GND	9-0000





IC-H5 LS193


9-8HPF


11-AFH8





